{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["SONARDYNE  LRT"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"SONARDYNE  LRT","index":0,"n_rows":41,"n_cols":12,"rows_kept":41,"cut":false,"hidden":false,"merged":[[20,1,20,8],[21,1,21,8],[22,1,22,8],[30,1,30,9],[30,10,30,11],[27,1,27,8],[31,1,31,9],[31,10,31,11],[23,1,23,8],[24,1,24,8],[25,1,25,8],[26,1,26,8],[28,1,28,8],[29,1,29,11],[3,6,3,10],[4,6,4,10],[6,1,6,2],[6,3,6,4],[6,6,6,7],[6,8,6,9],[17,1,17,8],[18,1,18,8],[19,1,19,8],[9,6,9,7],[9,8,9,9],[12,1,12,8],[13,1,13,8],[14,1,14,8],[16,1,16,8],[15,1,15,8],[7,1,7,2],[7,3,7,4],[7,6,7,7],[7,8,7,9],[8,1,8,2],[8,3,8,4],[8,6,8,7],[8,8,8,9],[38,1,38,9],[38,10,38,11],[40,1,43,1],[40,2,43,11],[32,1,32,9],[32,10,32,11],[33,1,33,9],[33,10,33,11],[34,1,34,9],[34,10,34,11],[35,1,35,9],[35,10,35,11],[36,1,36,9],[36,10,36,11],[37,1,37,9],[37,10,37,11]]}
[]
[]
[]
[null,null,null,null,null,null,"SONARDYNE  LRT"]
[null,null,null,null,null,null,"INSPECTION  CHECKLIST"]
[]
[null,"Customer: ",null,null,null,null,"Date of Inspection: ",null,{"$f":"NOW()","v":"2021-02-17T14:55:25.610"}]
[null,"Job Number: ",null,null,null,null,"Pre/Post Rental: "]
[null,"Asset Number: ",null,null,null,null,"Serial Number: "]
[null,null,null,null,null,null,"Checked by: ",null,{"$f":"Username()","v":"finlay.milne"}]
[]
[null,null,null,null,null,null,null,null,null,"PASS","FAIL","N/A"]
[null,"Check unit for physical damage paying particular attention to the transducer."]
[null,"Remove unit from case and ensure is clean, clean with fresh water if needed (Post rental only)."]
[null,"Meter battery and ensure it exceeds 14.0VDC when not under load."]
[null,"Connect battery back into LRT tube and reassembly unit."]
[null,"Connect unit to LCU test loop and program to address of choice (between 001 & 401). Record address."]
[null,"Press the test/range button on the LCU & ensure unit responds with “pass”"]
[null,"Test battery voltage of LRT via deck unit and record voltage as LRT is now under load\n(ensure exceeds 13.5 Volts)."]
[null,"If no nut is present change frequency to ‘Load’ and load nut as per manual. (This takes 60 seconds)"]
[null,"Disconnect test loop and plug transducer into LCU and put LRT and transducer in test tank."]
[null,"Change frequency to original setting and press program and load together for 1 second and repeat within 20 seconds. Ensure the nu is released correctly."]
[null,"Ensure release nut is in good condition."]
[null,"Grease and replace the nut using ‘Load’ option as above."]
[null,"Ensure red pressure relief valve is free to release & check it is correctly seated."]
[null,"Ensure LRT is labelled with correct address and frequency + Record:"]
[null,"Disconnect battery (post rental only)."]
[null,"Record Battery Pack Voltage under load:"]
[null,"Ensure unit is clean & presentable."]
[]
[null,"Package unit in transit case complete with:",null,null,null,null,null,null,null,null,"Tick as required"]
[null,"1 x Sonardyne LRT Release Transponder"]
[null,"1 x Release Nut"]
[null,"2 x Shackle"]
[null,"1 x USB Stick containing Manuals"]
[null,"1 x Set of spare Batteries"]
[null,"1 x Battery MSDS"]
[null,"2 x Spare Release Blocks"]
[null,"1 x Transit Case"]
[]
[null,"Comments:"]