{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":52,"n_cols":12,"rows_kept":52,"cut":false,"hidden":false,"merged":[[39,2,39,9],[38,2,38,9],[37,2,37,9],[36,2,36,9],[35,2,35,9],[43,2,43,9],[42,2,42,9],[41,2,41,9],[40,2,40,9],[40,10,40,11],[41,10,41,11],[42,10,42,11],[48,2,48,9],[47,2,47,9],[46,2,46,9],[45,2,45,9],[44,2,44,9],[51,1,54,1],[51,2,54,11],[49,10,49,11],[49,2,49,9],[50,1,50,11],[47,10,47,11],[48,10,48,11],[43,10,43,11],[44,10,44,11],[45,10,45,11],[46,10,46,11],[39,10,39,11],[37,10,37,11],[33,10,33,11],[38,10,38,11],[36,10,36,11],[35,10,35,11],[34,10,34,11],[3,6,3,10],[4,6,4,10],[6,1,6,2],[6,3,6,4],[6,6,6,7],[6,8,6,9],[16,1,16,8],[17,1,17,8],[18,1,18,8],[9,6,9,7],[9,8,9,9],[12,1,12,8],[13,1,13,8],[14,1,14,8],[15,1,15,8],[7,1,7,2],[7,3,7,4],[7,6,7,7],[7,8,7,9],[8,1,8,2],[8,3,8,4],[8,6,8,7],[8,8,8,9],[29,10,29,11],[22,1,22,8],[23,1,23,8],[24,1,24,8],[25,1,25,8],[26,1,26,8],[29,2,29,9],[28,1,28,11],[30,10,30,11],[31,2,31,9],[31,10,31,11],[32,2,32,9],[32,10,32,11],[30,2,30,9],[33,2,33,9],[34,2,34,9],[19,1,19,8],[20,1,20,8],[21,1,21,8],[27,1,27,8]]}
[]
[]
[]
[null,null,null,null,null,null,"Hemisphere VS330"]
[null,null,null,null,null,null,"INSPECTION  CHECKLIST"]
[]
[null,"Customer: ",null,null,null,null,"Date of Inspection: ",null,{"$f":"NOW()","v":"2021-05-25T12:30:29.080"}]
[null,"Job Number: ",null,null,null,null,"Pre/Post Rental: "]
[null,"Asset Number: ",null,null,null,null,"Serial Number: "]
[null,null,null,null,null,null,"Checked by: ",null,{"$f":"Username()","v":"Unique"}]
[]
[null,null,null,null,null,null,null,null,null,"PASS","FAIL","N/A"]
[null,"Check system for physical damage, paying attention to connectors, threads, and antenna faces."]
[null,"Meter and Megger antenna cables and check for physical damage."]
[null,"PAT test power supply if required."]
[null,"Ensure USB has up to date Software and Manuals."]
[null,"Set up the antennas with a clear view of the sky, 1 or 2M separation. Measure the antenna seperation to within accuracy of mm if possible. This will need to be entered into ant seperation section of software. Orientate connectors in the same direction if possible for highest accuracy."]
[null,"Connect antenna cables and power to the VS330 Receiver, connecting Primary RF to the A43 antenna. Ensure receiver is facing in the direction of the Primary antenna."]
[null,"Power up the system and select Config Wizard > Use Previous > Unique.\nIf no presets are available, create one with the following settings:\nDiff > SBAS             \nData Port A > GPGGA, GPZDA - 1 Hz – 9600 Baud\nData Port B > GPHDT – 10Hz – 9600 Baud\nAiding Features > Gyroaid - No, Tiltaid – No\nBias, Neg, Tilt > Heading  - 0, Pitch – 0, Neg Tilt – No, Level Op – No\nAnt. Sep > What value you measured as ant seperation.\nPitch/Roll > Pitch"]
[null,"If operating correctly front LEDs should settle as follows:\nPOWER ● , PRIM GPS ● , SEC GPS ● , DIFF ● , HEADING ●\nNote the computed value will not be populated in the VS330 receiver software or the Sec / Heading LED on front of unit come on if a wrong ant seperation value is entered in the manual ant sep section."]
[null,"Select Vector > Display and ensure heading is coming in. Antenna cables can be swapped over to temporarily switch heading +180 degrees and ensure function."]
[null,"Select GNSS > Position Status and ensure position is accurate – Lat: 57⁰, Long: -2⁰."]
[null,"Ensure satellite information is seen in the GPS Sats and GLONASS Sats menus."]
[null,"Connect serial cables to Ports A and B and ensure data is correctly outputting to PC."]
[null,"Open the PocketMax software and ensure the Ports can be linked to see all data together."]
[null,"Check the USB Logging function: Data Logging > Start Recording > End, and check the data is good."]
[null,"Check the function of the PPS Port."]
[null,"Ensure the unit is clean and presentable."]
[]
[null,"Qty","Package unit in transit case complete with:",null,null,null,null,null,null,null,"Tick as required"]
[null,1,"Hemisphere VS330 Vector Sensor"]
[null,2,"10m Antenna Cable"]
[null,1,"DC Power Lead - Lemo Type"]
[null,1,"24Vdc Adaptor"]
[null,1,"UK Mains Lead"]
[null,1,"EU Adaptor"]
[null,1,"US Adaptor"]
[null,2,"Antenna Adaptor"]
[null,1,"PPS Cable"]
[null,1,"9 Way D Type Lead"]
[null,1,"USB stick c/w Software & Manuals"]
[null,2,"Mounting Brackets (Installed)"]
[null,1,"A43 Antenna"]
[null,1,"A42 Antenna"]
[null,3,"Spare Fuses"]
[null,1,"Operations Manual"]
[null,1,"Spec Sheet"]
[null,1,"Quick Start Sheet"]
[null,2,"GPS Magnetic Mount"]
[null,2,"Extension Rods"]
[]
[null,"Comments:"]