{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Applanix POS MV"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Applanix POS MV","index":0,"n_rows":69,"n_cols":12,"rows_kept":69,"cut":false,"hidden":false,"merged":[[19,1,19,8],[20,1,20,8],[21,1,21,8],[31,1,31,8],[25,1,25,8],[27,1,27,8],[29,1,29,8],[28,1,28,8],[24,1,24,8],[41,1,41,11],[33,1,33,8],[34,1,34,8],[35,1,35,8],[36,1,36,8],[37,1,37,8],[38,1,38,8],[39,1,39,8],[40,1,40,8],[32,1,32,8],[22,1,22,8],[23,1,23,8],[26,1,26,8],[30,1,30,8],[7,1,7,2],[7,3,7,4],[7,6,7,7],[7,8,7,9],[8,1,8,2],[8,3,8,4],[8,6,8,7],[8,8,8,9],[16,1,16,8],[17,1,17,8],[18,1,18,8],[9,6,9,7],[9,8,9,9],[12,1,12,8],[13,1,13,8],[14,1,14,8],[15,1,15,8],[3,6,3,10],[4,6,4,10],[6,1,6,2],[6,3,6,4],[6,6,6,7],[6,8,6,9],[42,2,42,9],[51,2,51,9],[51,10,51,11],[49,2,49,9],[49,10,49,11],[50,2,50,9],[43,2,43,9],[48,10,48,11],[43,10,43,11],[44,2,44,9],[44,10,44,11],[45,2,45,9],[45,10,45,11],[46,2,46,9],[47,2,47,9],[42,10,42,11],[52,10,52,11],[50,10,50,11],[46,10,46,11],[52,2,52,9],[48,2,48,9],[47,10,47,11],[53,10,53,11],[54,10,54,11],[55,10,55,11],[61,2,61,9],[56,2,56,9],[57,2,57,9],[58,2,58,9],[59,2,59,9],[60,2,60,9],[59,10,59,11],[60,10,60,11],[61,10,61,11],[56,10,56,11],[55,2,55,9],[53,2,53,9],[54,2,54,9],[68,1,71,1],[68,2,71,11],[65,10,65,11],[66,10,66,11],[62,10,62,11],[63,10,63,11],[64,10,64,11],[62,2,62,9],[63,2,63,9],[64,2,64,9],[65,2,65,9],[66,2,66,9],[57,10,57,11],[58,10,58,11]]}
[]
[]
[]
[null,null,null,null,null,null,"Applanix POS MV"]
[null,null,null,null,null,null,"Inspection Checklist"]
[]
[null,"Customer: ",null,null,null,null,"Date of Inspection: ",null,{"$f":"NOW()","v":"2020-09-17T09:30:43.040"}]
[null,"Job Number: ",null,null,null,null,"Pre/Post Rental: "]
[null,"Asset Number: ",null,null,null,null,"Serial Number: "]
[null,null,null,null,null,null,"Checked by: "]
[]
[null,null,null,null,null,null,null,null,null,"PASS","FAIL","N/A"]
[null,"Record asset number of IMU:"]
[null,"Record asset number of IMU Cable:"]
[null,"Record asset number of PCS:"]
[null,"Record asset number of Laptop:"]
[null,"Record asset number of POSPac Dongle:"]
[null,"Check system for damage paying special attention to IMU and connectors."]
[null,"If required, PAT test topside and laptop charger."]
[null,"Carry out insulation and continuity on IMU cable & antenna cables and check for damage."]
[null,"Assemble system as per procedure and measure offsets."]
[null,"Acquire a suitable laptop and ensure it has the latest software version. Note that authorisations codes are required if swapping the PCS with different types of IMU."]
[null,"Ensure the laptop IP address is set to: 192.168.53.99, Subnet mask: 255.255.255.0 and label unit as such."]
[null,"Ensure the POWER ON and RESET buttons on the PCS front panel are operational.\nIf not then it can be case that client has changed the power on option via the \nPOSLOADER software. In that case reset it to correct option to enable these buttons."]
[null,"If the client has set the system to another IP address and subnet mask then the user can determine what this is by connecting a serial cable from Comm3 at 9600 baud rate on the standard orange PCS to a laptop serial port with a terminal program like terraterm installed.\nPower cycle the system and after a short time the current system IP address will be displayed in the hyperterminal. Note if it's a SFF System then it will be the Fan out cable marked \"Com\" on it's IO1 port at 19200 that shows the current IP address and Subnet mask upon power up."]
[null,"Open PosView Software and connect to PCS (PCS default IP is: 192.168.53.100)."]
[null,"Set unit to factory default settings."]
[null,"Ensure satellites can be seen in the GNSS Data window."]
[null,"Ensure in the View > Statistics section of the POSVIEW software that the PCS is set to use the correct type of IMU that is being used with it. For example it should be set for type 45 if a wavemaster IMU is being used or type 65 if an Oceanmaster type is being used.\nIf the incorrect type is shown here then it can be set correctly via the POSCONFIG software (correct licence code is on Unique network to set each PCS to desired IMU type)"]
[null,"Ensure system completes calibration and ensure all appropriate lights are green in the \"Fault Detection\" section. And no bad frames in the IMU."]
[null,"Setup system for USB and Ethernet logging. Ensure correct USB memory is detected and the unit logs data correctly (Must use the Yellow 8GB stick provided with system). Firstly check it can log when stick is in usb port at front of PCS then also with it in USB port at rear of PCS."]
[null,"Check pitch, roll, heading and heave function correctly."]
[null,"Check comms are maintained while flexing the IMU cable (wet end IMU cable neck can become intermittent which usually results in an IMU Failure message in the POSVIEW software)."]
[null,"Check the PPS port on the PCS."]
[null,"Check the input + output functions of comm ports 1 - 5. (Test inputs with external GPS if available)."]
[null,"Take screenshots when testing of the view statistics page + also main page when all data\n is coming in and light are green in the POSVIEW software. Save these in network asset folder."]
[null,"Ensure firmware version, PCS IP address + subnet mask plus type of IMU PCS is set for are all labelled on the PCS (Eg Firmware V10.21, IP 192.168.53.100, subnet 255.255.255.0 and \"System is set for Oceanmaster Type 65 IMU Use\")"]
[null,"Record PCS firmware version:"]
[null,"Record POSVIEW Software Version used and on USB with system:"]
[null,"Record PCS IP address AND subnet mask:"]
[null,"Ensure unit is clean and presentable."]
[]
[null,"Qty","Package unit in transit case complete with:",null,null,null,null,null,null,null,"Tick as required"]
[null,1,"Applanix POSMV Surface Unit (V5, PCS-84)"]
[null,1,"POSMV Surfmaster/Wavemaster/Oceanmaster IMU"]
[null,3,"Mains Lead"]
[null,1,"RJ45 Ethernet cable"]
[null,2,"Trimble GPS Antenna (Record Model and Serial Number of antennas):"]
[null,2,"9WF-9WF RS232 cables"]
[null,1,"BNC PPS Lead"]
[null,1,"USB Pen Drive c/w software and manuals"]
[null,1,"Yellow 8GB Applanix USB Drive"]
[null,1,"Blue 4GB Applanix USB Drive"]
[null,2,"Antenna Mouting Brackets c/w fittings"]
[null,2,"Black Plastic threaded antenna mounting rods"]
[null,1,"Alignment Bar c/w Screws"]
[null,1,"Black Plastic Transit Case"]
[]
[null,1,"POSMV IMU Cable - IP68 (State length):"]
[null,2,"10 Metre Antenna Cable"]
[null,2,"15 Metre Antenna Cable"]
[null,2,"25 Metre Antenna Cable"]
[null,2,"30 Metre Antenna Cable"]
[null,2,"40 Metre Antenna Cable"]
[null,2,"50 Metre Antenna Cable"]
[null,2,"TNC Adaptor"]
[null,1,"Black Plastic Transit Case"]
[]
[null,"Comments:"]