{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["R2sonic 2024 Multibeam Sonar"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"R2sonic 2024 Multibeam Sonar","index":0,"n_rows":81,"n_cols":12,"rows_kept":81,"cut":false,"hidden":false,"merged":[[46,1,46,9],[45,10,45,11],[47,1,47,9],[46,10,46,11],[48,1,48,9],[47,10,47,11],[43,1,43,9],[43,10,43,11],[44,1,44,9],[44,10,44,11],[45,1,45,9],[3,6,3,10],[4,6,4,10],[6,1,6,2],[6,3,6,4],[6,6,6,7],[6,8,6,9],[7,1,7,2],[7,3,7,4],[7,6,7,7],[7,8,7,9],[8,1,8,2],[8,3,8,4],[8,6,8,7],[8,8,8,9],[21,1,21,8],[9,6,9,7],[9,8,9,9],[12,1,12,8],[13,1,13,8],[14,1,14,8],[15,1,15,8],[16,1,16,8],[17,1,17,8],[18,1,18,8],[19,1,19,8],[20,1,20,8],[22,1,22,8],[23,1,23,8],[24,1,24,8],[25,1,25,8],[26,1,26,8],[27,1,27,8],[41,1,41,11],[31,1,31,8],[32,1,32,8],[33,1,33,8],[34,1,34,8],[35,1,35,8],[36,1,36,8],[37,1,37,8],[28,1,28,8],[29,1,29,8],[30,1,30,8],[42,1,42,9],[42,10,42,11],[38,1,38,8],[39,1,39,8],[40,1,40,8],[48,10,48,11],[50,1,50,9],[49,10,49,11],[51,1,51,9],[50,10,50,11],[49,1,49,9],[52,1,52,9],[51,10,51,11],[53,1,53,9],[52,10,52,11],[54,1,54,9],[53,10,53,11],[54,10,54,11],[56,1,56,9],[55,10,55,11],[57,1,57,9],[56,10,56,11],[57,10,57,11],[59,1,59,9],[58,10,58,11],[59,10,59,11],[55,1,55,9],[64,1,67,1],[60,1,60,9],[62,1,62,9],[60,10,60,11],[58,1,58,9],[61,1,61,9],[61,10,61,11],[62,10,62,11],[64,2,67,11]]}
[]
[]
[]
[null,null,null,null,null,null,"R2sonic 2024 Multibeam Sonar"]
[null,null,null,null,null,null,"INSPECTION  CHECKLIST"]
[]
[null,"Customer: ",null,null,null,null,"Date of Inspection: ",null,{"$f":"NOW()","v":"2019-06-03T09:52:08.340"}]
[null,"Job Number: ",null,null,null,null,"Pre/Post Rental: "]
[null,"Asset Number: ",null,null,null,null,"Serial Number: "]
[null,null,null,null,null,null,"Checked by: ",null,{"$f":"Username()","v":"kris.mikos"}]
[]
[null,null,null,null,null,null,null,null,null,"PASS","FAIL","N/A"]
[null,"Record asset number of receiver:"]
[null,"Record asset number of projector:"]
[null,"Record asset number of deck cable:"]
[null,"Record asset number of pole mount bracket:"]
[null,"Record asset number of Sonar Interface Module (SIM):"]
[null,"Check unit for physical damage paying particular attention projector & receive array."]
[null,"Take photographs of projector & receive array and in particular any existing damage."]
[null,"Check connectors for corrosion/damage – includes removing protective plate covering the two connectors on the receiver"]
[null,"Check full length of deck cable for damage"]
[null,"Carry out insulation & continuity test on all cables. Ensure there is no charge left in cables before plugged into Sonar Head or SIM Box."]
[null,"Carry out PAT test on SIM if required."]
[null,"Install system in pole mount bracket if one is available + Connect the system up as per manual (and Unique Test Procedure)"]
[null,"Deploy bracket with the sonar heads and deck cable installed into the test tank to the point the bracket is fully submerged."]
[null,"Check R2 SONIC website for latest Software + Firmware Updates & record:"]
[null,"Set IP address of laptop to 10.0.1.102 and subnet mask: 255.0.0.0. Copy R2sonic software folder to C Drive of laptop being used and open the Sonic Control 2000 software."]
[null,"For simplicity – Connect an RS232 signal with $GPZDA at 9600 baud to “GPS” port on SIM using a simulator software like “Generate” , TSS1 Motion at 115200 baud min 25hz(ideally 50hz) update rate to motion port, Minisvs data (format 1234.567 M/S, baud 9600 and update rate “fast as possible”) to SVS port + at 1PPS signal via bnc cable to pps port on SIM"]
[null,"Connect Ethernet Cable From “Data” ethernet port on Sim to Laptop LAN Port and then switch on Sim"]
[null,"In Sonic Control Software > Settings > Sonar Settings Ensure Sonar Power Tick box is Ticked."]
[null,"In Settings > Network Settings Click the Discover button. The serial number/type of the SIM and the Sonar Head should appear in the box below to confirm comms with the whole system is established."]
[null,"In Settings > Sensor Settings Ensure the correct baud rate is selected for GPS (ZDA time string not actually GPS position), motion and minisvs then click apply. All leds on software bottom left taskbar should be green to confirm relevant inputs being received and expected."]
[null,"SV data might not come through until the sound velocity tickbox is unticked within Settings > Ocean Settings window. It will probably be required to unlock laptop bottom taskbar and drop taskbar to right of screen to reveal this window as it seems like a software glitch."]
[null,"Ensure comms to the unit are stable – ensure network speed is 1GB."]
[null,"In order to get the system to track the tank bottom and sides it will likely be necessary to click the Enable gates tick box on main software page then set the min gate to 0.0M and max gate to 1.0M. Also set range to least value (2M)\nTake Screenshot clearly showing the system tracking the bottom and sides of the test tank in a range of different frequencies. Save Screenshot is AX asset folder"]
[null,"Ensure In Status > System Status that the time, motion and sv all update correctly in this window. Ensure that the head and sim model, serial number and firmware version lines are all populated automatically by the system. Note TX voltage will be around 0.7V when system is set to min power and around 38V or 45V with full power on depending the version of the projector used.\nTake Screenshots Of Status Window When all inputs are interfaced into SIM and TX power is set to full. Save screenshots to AX Asset Folder"]
[null,"Ensure the full range of frequencies are available for selection – 170 to 450 KHz"]
[null,"Check operation in UHR mode (if applicable). This will likely be a 700khz option in the sonar settings window."]
[null,"In Help  > Options record the options that are enabled / licenced on the system and save screenshot of this to AX asset folder:"]
[null,"If unit is going to be used in dual head test with a second unit. The Ops Manual describes how to interface this."]
[null,"Ensure unit is clean & presentable."]
[]
[null,"Package unit in transit case complete with:",null,null,null,null,null,null,null,null,"Tick as required"]
[null,"R2Sonic 2024 Receiver Assembly"]
[null,"R2Sonic 2024 SIM Box"]
[null,"Projector to Receiver Cable"]
[null,"1 x LPIL-12-FS or MCOM12F Subsea Tail Dependant on revision of 2024 Receiver Being Tested."]
[null,"3 X Mains Leads (UK/EU/US)"]
[null,"3 X 9WF-9WF D Type RS232 Cables"]
[null,"1 X BNC Cable"]
[null,"1 x R2sonic Software + Manuals USB Stick – record version:"]
[null,"1 x RJ45 Gigabit Ethernet Cable"]
[null,"1 x Quick Start Guide"]
[null,"1 x Roll of PTFE Tape"]
[null,"Receiver Mounting Kit – Contains;"]
[null,"8 x M8 Nylon Insulators, \n8 x M8 Plain Washers, \n8 x M8 Spring Washers, \n8 x M8 Nuts"]
[null,"Projector Mounting Kit – Contains;"]
[null,"2 x Projector Standoff Mounts, \n4 x M8 Nylon Insulators, \n4 x M8 x 60 Socket Head Cap Screws, \n4 x M8 Plain Washers, \n4 x M8 Spring Washers"]
[null,"SVS Mounting kit – Contains; "]
[null,"1 x Cap, \n1 x Base, \n4 x M6 Washers\n4 x M6 x 35 Socket Head Cap Screw, \n4 x M6 x 16 Countersunk Head Screw,\n"]
[null,"Cable Clamp Kit (new style heads) – Contains;"]
[null,"1 x Bottom Clamp, \n1 x Top Clamp, \n4 x M4 x 30 Crosshead Screws, \n6 x M4 Plain Washer, \n6 x M4 Spring Washer, \n2 x M4 x 16 Crosshead Screws"]
[null,"R2Sonic 2024 Deck Cable"]
[]
[null,"Comments:"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Pre","Post","Both"]