{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Tritech Gemini 720is"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tritech Gemini 720is","index":0,"n_rows":59,"n_cols":12,"rows_kept":59,"cut":false,"hidden":false,"merged":[[37,1,37,8],[45,10,45,11],[28,1,28,8],[29,1,29,8],[31,1,31,8],[32,1,32,8],[34,1,34,8],[44,1,44,11],[41,1,41,8],[42,1,42,8],[43,1,43,8],[9,6,9,7],[9,8,9,9],[12,1,12,8],[14,1,14,8],[16,1,16,8],[3,6,3,10],[4,6,4,10],[6,1,6,2],[6,3,6,4],[6,6,6,7],[6,8,6,9],[51,2,51,9],[45,2,45,9],[54,2,54,9],[54,10,54,11],[52,2,52,9],[52,10,52,11],[53,2,53,9],[46,2,46,9],[51,10,51,11],[46,10,46,11],[47,2,47,9],[47,10,47,11],[48,2,48,9],[7,6,7,7],[7,8,7,9],[8,1,8,2],[8,3,8,4],[8,6,8,7],[8,8,8,9],[7,1,7,2],[7,3,7,4],[58,1,61,1],[58,2,61,11],[22,1,22,8],[21,1,21,8],[18,1,18,8],[19,1,19,8],[48,10,48,11],[49,2,49,9],[50,2,50,9],[50,10,50,11],[56,10,56,11],[56,2,56,9],[55,10,55,11],[53,10,53,11],[49,10,49,11],[55,2,55,9],[13,1,13,8],[33,1,33,8],[39,1,39,8],[38,1,38,8],[40,1,40,8],[30,1,30,8],[17,1,17,8],[15,1,15,8],[23,1,23,8],[24,1,24,8],[20,1,20,8],[25,1,25,8],[26,1,26,8],[27,1,27,8],[35,1,35,8],[36,1,36,8]]}
[]
[]
[]
[null,null,null,null,null,null,"Tritech Gemini 720is"]
[null,null,null,null,null,null,"Inspection Checklist"]
[]
[null,"Customer: ",null,null,null,null,"Date of Inspection: ",null,{"$f":"NOW()","v":"2019-08-16T09:10:45.350"}]
[null,"Job Number: ",null,null,null,null,"Pre/Post Rental: "]
[null,"Asset Number: ",null,null,null,null,"Serial Number: "]
[null,null,null,null,null,null,"Checked by: ",null,{"$f":"Username()","v":"drummond.hosea"}]
[]
[null,null,null,null,null,null,null,null,null,"PASS","FAIL","N/A"]
[null,"Check unit for physical damage paying particular attention to the transmitter, receiver and sound velocity probe."]
[null,"Remove the blue protective fairing on the front of the sonar and check for any damage beneath. Install fairing back on once check is completed."]
[null,"Check connector bulkhead connector of unit for corrosion/damage."]
[null,"Check condition of both anodes. Clean or replace if required."]
[null,"Carry out insulation & continuity test on all subsea cables including the 8 pin pigtail provided with the system."]
[null,"Record Sonar Asset Number:"]
[null,"Record VDSL Topside Unit / Adapter Asset Number:"]
[null,"Record Ethernet Topside Unit / Adapter Asset Number:"]
[null,"If required, PAT test PSU and AC Power Lead"]
[null,"Check Technical support - Software section of Tritech website and check if there is an updated version of the software for the Gemini. Dowload and install on laptop if applicable."]
[null,"Connect 720is sonar to its black ethernet deck lead and then top end of ethernet deck lead to the Tritech Ethernet surface unit."]
[null,"Connect an ethernet cable from the surface unit to a laptop with the latest Tritech Gemini softare on it."]
[null,"Set laptop IP address to 192.168.2.xxx where xxx is not 201 as that is the default IP address of the sonar."]
[null,"Deploy sonar in test tank so that it can \"see\" 3 sides of the tank clealy."]
[null,"Apply power to Ethernet topside box and open the Gemini software"]
[null,"It may initially be required to ensure in the advanced tab and configuration dropdown option that \"imager\" is set rather than \"profiler\"."]
[null,"Sonar information should be shown in the lower area of window, click the online button at the top and the main sonar screen should now show data."]
[null,"The lower window should show the sonar hardware information, versions and ethernet information in GREEN to confirm connection is established and working."]
[null,"If the sonar firmware needs upgraded - eg an updated version of software has just been installed that includes firmware updated version - the firmware displayed in the software won't be in green.                                                                                                                                           There will be an option to update it from within the software - update as necessary (the firmware version then shown will be green to confirm its been updated to required version)."]
[null,"Change range and gain to get a good image of the test tank sides. Adjust sonar position in tank as required to get the solid image."]
[null,"Ensure the \"measured sound velocity\" reading in the top right of sonar screen is displyed and verify its accuracy by comparing it to a freshly calibrated sv sensor in the tank at the same time."]
[null,"Take screenshot of system that shows the adanced tab in the software - tracking tank sides, showing the sv value and showing system software/firmware/connection methods at bottom of page."]
[null,"Disconnect unit from software, power down system and recover from test tank. Set Ethernet surface unit and its deck lead aside and get the VDSL surface unit and its deck lead."]
[null,"Connect the deck lead wet end to sonar head and topside end to VDSL topside unit. Connect power to topside unit and ethernet cable from it to the test laptop. Redeploy sonar back in test tank."]
[null,"Repeat test in same manner as with ethernet topside box but this time when connected in the software note in the advanced tab and bottom of page it will read VDSL in link type instead of ethernet."]
[null,"Take screenshot of system that shows the adanced tab in the software - tracking tank sides, showing the sv value and showing system software/firmware/connection methods at bottom of page."]
[null,"Record Software Version on sonar:"]
[null,"Record Firmware Version on sonar:"]
[null,"Record IP address and subnet mask of Sonar:"]
[null,"Disconnect system in software, power in down and remove from test tank."]
[null,"Dry system, ensure all items and present and pack away in box."]
[null,"Normally, the VDSL Surface Adapter and deck lead are kept seperately in Unique checked kit area and only sent with the sonars if clinet specifically requests them."]
[]
[null,"Qty","Package unit in transit case complete with:",null,null,null,null,null,null,null,"Tick as required"]
[null,1,"10M ethernet deck lead"]
[null,1,"Ethernet surface topside / adapter"]
[null,1,"10M VDSL topside lead"]
[null,1,"VDSL surface topside / adapter"]
[null,1,"Ethernet RJ45-RJ45 Cable"]
[null,1,"8 Pin Burton Tail (MUST be correct type for Gemini Ethernet comms NOT standard connector)"]
[null,1,"USB Stick containig latest Gemini software and manuals"]
[null,1,"Allen key"]
[null,1,"Tritech Topside Box PSU"]
[null,3,"AC Power Leads (UK/EU/US)"]
[null,1,"Transit Case"]
[]
[null,"Comments:"]