{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":41,"n_cols":12,"rows_kept":41,"cut":false,"hidden":false,"merged":[[22,1,22,8],[20,1,20,8],[28,10,28,11],[33,10,33,11],[34,10,34,11],[21,1,21,8],[24,1,24,8],[25,1,25,8],[26,1,26,8],[27,1,27,8],[29,10,29,11],[30,2,30,9],[30,10,30,11],[31,2,31,9],[31,10,31,11],[32,2,32,9],[33,2,33,9],[17,1,17,8],[7,1,7,2],[7,3,7,4],[7,6,7,7],[7,8,7,9],[8,1,8,2],[8,3,8,4],[8,6,8,7],[8,8,8,9],[35,2,35,9],[35,10,35,11],[36,2,36,9],[29,2,29,9],[3,6,3,10],[4,6,4,10],[6,1,6,2],[6,3,6,4],[6,6,6,7],[6,8,6,9],[18,1,18,8],[19,1,19,8],[9,6,9,7],[9,8,9,9],[12,1,12,8],[16,1,16,8],[40,1,43,1],[40,2,43,11],[14,1,14,8],[13,1,13,8],[23,1,23,8],[15,1,15,8],[38,2,38,9],[38,10,38,11],[39,10,39,11],[36,10,36,11],[32,10,32,11],[39,2,39,9],[34,2,34,9],[28,2,28,9],[37,2,37,9],[37,10,37,11]]}
[]
[]
[]
[null,null,null,null,null,null,"Sonardyne WSM 8270 + 8271"]
[null,null,null,null,null,null,"Inspection Checklist"]
[]
[null,"Customer: ",null,null,null,null,"Date of Inspection: ",null,{"$f":"NOW()","v":"2020-01-22T11:51:46.720"}]
[null,"Job Number: ",null,null,null,null,"Pre/Post Rental: "]
[null,"Asset Number: ",null,null,null,null,"Serial Number: "]
[null,null,null,null,null,null,"Checked by: ",null,{"$f":"Username()","v":"drummond.hosea"}]
[]
[null,null,null,null,null,null,null,null,null,"PASS","FAIL","N/A"]
[null,"Asset number of beacon:"]
[null,"Asset number of Charger/Comms unit:"]
[null,"Inspect beacon transducer for leaks or cuts."]
[null,"Inspect transducer guard of beacon (8271 beacon only)"]
[null,"Check beacon off/on/off switch is working. Each position a click should be felt when the switch is position from off-on-off position."]
[null,"Connect to beacon using the WSM Terminal V3.01.05 software. Ensure beacon can be set to different addresses as there has been historic cases where a beacon was stuck on one address."]
[null,"Fully charge the beacon as per the instructions in the 8270 or 8271 Ops manual."]
[null,"If possible check the beacon in the test tank with a USBL system. If no USBL system is available, check it with either the PAM tester topside unit. Test at HPR and Sonardyne Quickset addresses."]
[null,"Via the WSM Terminal software, ensure depth is set to off and by default power is set to low and gain set to high."]
[null,"Ensure the beacon has labels on it stating the address its been left set in. By default it should be set to a Sonardyne Quickset addrees - eg A1, A2 or A3."]
[null,"Connect to beacon using the 6G Utilities software, carry out the tests and then create the 6G report from the software. Print off 6G report, put in beacon box and also save a copy on the AX asset folder."]
[null,"Ensure beacon is fully charged before packing away."]
[null,"Ensure beacon switch is set to OFF position before packing away."]
[null,"Record address beacon is set to:"]
[null,"Record version of WSM Terminal used:"]
[null,"Ensure usb stick with system has 8270/8271 ops manual and WSM Terminal V3.01.05 on it. Ensure the version of WSM terminal on the usb stick works."]
[null,"Qty","Package unit in transit case complete with:",null,null,null,null,null,null,null,"Tick as required"]
[null,1,"Sonardyne Beacon"]
[null,1,"5WF Microsubcon dummy plug and female locking collar."]
[null,1,"WSM 7972 Comms/charger unit."]
[null,1,"9WM-9WF Straight through RS232 cable"]
[null,1,"UK AC Power Lead"]
[null,1,"EU AC Power Lead"]
[null,1,"US AC Power Lead"]
[null,1,"30VDC 0.5A Sonardyne DC Power Supply"]
[null,1,"USB stick containg software and manuals"]
[null,1,"MSDS Sheets for beacon batteries."]
[null,1,"Blue plastic carrycase"]
[null,"Comments:"]