{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":45,"n_cols":12,"rows_kept":45,"cut":false,"hidden":false,"merged":[[41,10,41,11],[17,1,17,8],[40,2,40,9],[41,2,41,9],[21,1,21,8],[22,1,22,8],[23,1,23,8],[32,1,32,8],[33,1,33,8],[34,1,34,8],[35,1,35,11],[37,10,37,11],[38,2,38,9],[38,10,38,11],[39,2,39,9],[39,10,39,11],[36,10,36,11],[7,1,7,2],[7,3,7,4],[7,6,7,7],[7,8,7,9],[8,1,8,2],[8,3,8,4],[8,6,8,7],[8,8,8,9],[16,1,16,8],[18,1,18,8],[19,1,19,8],[9,6,9,7],[9,8,9,9],[12,1,12,8],[13,1,13,8],[14,1,14,8],[15,1,15,8],[12,9,12,11],[3,6,3,10],[4,6,4,10],[6,1,6,2],[6,3,6,4],[6,6,6,7],[6,8,6,9],[44,1,47,1],[44,2,47,11],[20,1,20,8],[26,1,26,8],[31,1,31,8],[40,10,40,11],[42,2,42,9],[36,2,36,9],[37,2,37,9],[42,10,42,11],[24,1,24,8],[25,1,25,8],[27,1,27,8],[28,1,28,8],[29,1,29,8],[30,1,30,8]]}
[]
[]
[]
[null,null,null,null,null,null,"c-Node Mini-S Transponder"]
[null,null,null,null,null,null,"INSPECTION  CHECKLIST"]
[]
[null,"Customer: ",null,null,null,null,"Date of Inspection: ",null,{"$f":"NOW()","v":"2019-10-08T15:08:43.030"}]
[null,"Job Number: ",null,null,null,null,"Pre/Post Rental: "]
[null,"Asset Number: ",null,null,null,null,"Serial Number: "]
[null,null,null,null,null,null,"Checked by: ",null,{"$f":"Username()","v":"chris.marr"}]
[]
[null,null,null,null,null,null,null,null,null,"PASS","FAIL","N/A"]
[null,"Record asset number of charger:"]
[null,"PAT test charger."]
[null,"Check unit for physical damage paying particular attention to the transducer."]
[null,"Check connector & blanking plug for corrosion/damage."]
[null,"Connect unit to charger & ensure charging cycle completes."]
[null,"Carrly out insulation and continuity test on subsea tail"]
[null,"Check correct operation of the pressure relief vent to ensure there is no pressure build-up inside the unit."]
[null,"Using a TTC30 Test/Config unit, connect the transponder using the serial cable (make sure to use the supplied c-Node Mini-S adaptor cable). "]
[null,"In the Transponder Configuration window check that the cNode is set to an FSK channel(e.g.B54)."]
[null,"Check FSK address matches label on outside of unit & record:"]
[null,"Check Cymbal address matches label on outside of unit & record:"]
[null,"Pre hire only: If job is for multiple c-Nodes ensure there are no conflicting addresses."]
[null,"Connect the supplied transducer to the TTC30 and point towards the c-Nodes transducer face."]
[null,"Interrogate the unit on the FSK channel in both transponder and responder modes and ensure the indicator on the screen is flashing green."]
[null,"When returning to Transponder from Responder the unit will fail just leave it pinging for a while and it will function correctly again."]
[null,"Check parameters are correct using the \"Read Parameters\" function."]
[null,"Check all fitted sensors, list can be seen in the \"Transponder Configuration\" tab. "]
[null,"Using the \"Read Battery\" function ensure  the battery is at full charge."]
[null,"Change the unit to a Cymbal channel (e.g. M02) and interrogate using Transponder and Responder functions again. "]
[null,"Once complete change back to FSK channel (B Channels)."]
[null,"Remove test lead from c-node and leave blanking plug out this will turn off the unit."]
[null,"Ensure transit case has a suitable label for unit containing Lithium batteries (Miscellaneous Substances Class 9)."]
[null,"Ensure unit is clean & presentable, change labels if required."]
[]
[null,"Qty","Package unit in transit case complete with:",null,null,null,null,null,null,null,"Tick as required"]
[null,null,"MCIL8F Tail c/w Locking Ring"]
[null,null,"Blanking Plug c/w Locking Ring"]
[null,null,"MSDS Sheet"]
[null,null,"Manual "]
[null,null,"USB Stick containing Software & Manuals "]
[null,null,"Transit Case "]
[]
[null,"Comments:"]